**Silent Gliss 2810 Mono-control Vertical Louvre Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 2810 Mono-control Vertical Louvre Blind System,

 **Max size 127mm louvres - 5m wide x 4m high**

 **Max size 89mm louvres – 3.8m wide x 4m high**

**Finish** White (RAL 9016 Gloss) or Satin Silver annodised as standard

**Operation** Mono control chain operation, white nylon

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories**  a) 89mm / 127mm width louvres\*

b) Bottom weights with Link chain / Sewn in bottom weights\*

c) Chain retainer to be installed min 150cm above floor level to comply with BS EN 13120:2009

d) Top fix / face fix brackets\*

e) Option of 2614 recess profile for suspended ceiling applications

\*Delete as appropriate – please contact technical@waverley.co.uk or 01252 737973 for advice