**Silent Gliss 4840 Chain Operated Roller Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 4840 Heavy Duty Chain Operated Roller Blind System, **Max size 5m wide x 6m high (max 15 m2). Min width 50cm**

**Finish** Stainless steel brackets with white nylon bracket covers, hembar inWhite (RAL 9016 Gloss) powdercoat finish as standard

**Operation** Manual, stainless steel bead chain

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories** a) 80mm / 110mm diameter roller tube (Depending on blind width)

b) Adjustable height facility on brackets ensures perfect alignment of fabric cover

c) lift-assist spring for ease of operation

c) option of side guide wires

d) chain retainer to be installed min 150cm above floor level to comply with BS EN 13120:2009

Please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice