**Silent Gliss 4880 Electrically Operated Roller Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 4880 Large Electrically Operated Roller Blind System, **Max size 5m wide x 12m high (max 36 m2). Min width 72cm or 100cm depending on motor choice.** (Please contact us for advice).

**Finish Stainless steel brackets with white nylon bracket scovers, hembar in** White (RAL 9016 Gloss) powdercoat finish as standard

**Operation** Electrically operated with 230v Hardwired motor\* or 230v radio motor with integrated receiver for use with 9940 series controls (Wall switch, hand-held remotes etc)\*

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories** a) 80mm or 110mm diameter roller tube (Depending on blind width)

b) adjustable height facility on brackets ensures perfect alignment of fabric cover

c) option of side guide wires

\*Delete as appropriate – please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice