**Silent Gliss 4910 Chain Operated Roller Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 4910 Chain Operated Roller Blind System, **Max size 2.4m wide x 3m high (max 10 m2). Min width 60cm**

**Finish** Steel brackets with white nylon bracket covers, hembar inWhite (RAL 9016 Gloss) powdercoat finish as standard

**Operation** Manual, stainless steel bead chain

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories** a) 41mm diameter roller tube

b) option of side guide wires

d) option of two systems linked with intermediate bracket, each with their own control chain

e) option of continuous mounting profile , white powdercoat finish

f) chain retainer to be installed min 150cm above floor level to comply with BS EN 13120:2009

Please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice