**Silent Gliss 4960 Electrically Operated Roller Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 4960 Electrically Operated Roller Blind System, **Max size 2.4m wide x 4m high (max 9.6 m2). Min width 61cm or 83cm depending on motor choice.** (Please contact us for advice).

**Finish** Steel brackets with white nylon bracket covers, hembar inWhite (RAL 9016 Gloss) powdercoat finish as standard

**Operation** Electrically operated with 230v Hardwired motor\* or 230v radio motor with integrated receiver for use with 9940 series controls (Wall switch, hand-held remotes etc)\*

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories** a) 41mm diameter roller tube

b) option of continuous mounting profile, white powdercoat finish

c) option of side guide wires

d) option of two systems linked with intermediate bracket, driven by one motor

\*Delete as appropriate – please contact technical@waverley.co.uk or 01252 737973 for advice