**Weinor Vertitex II Vertical Awning System**

**Manufacturer** Weinor – www.weinor.com

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference \***Weinor Vertitex II Vertical Awning System with ZIP side channels, **Max size 6m wide x 3m drop. Max 15m²**

\*Weinor Vertitex II Vertical Awning System with guide wires, **Max size 6m wide x 3m drop. Max 14.4m²**

**Finish** All hardware in powdercoat finish to RAL….(choice of 47 standard colours selected from Weinor range)

**Operation** Electrically operated with 230v Hardwired motor\* or 230v radio motor with integrated receiver for use with BiEasy series controls (Wall switch, hand-held remotes, Wind & Sun sensor, motion sensors etc)\*

**Material** Fabric to be acrylic or polyester fabric selected from Weinor ‘My Collections’ range

\*Delete as appropriate – please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice