**ShadeTech RBL-C Manual Roller Blind**

**Manufacturer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham,

GU9 9PZ

Tel. 01252 737973

www.waverley.co.uk

Email sales@waverley.co.uk

**Reference** ShadeTech RBL-C Chain Operated manual Roller Blind System, 40mm/45mm diameter roller barrel. Max size 3.2m wide x 3.5m high

**Operation** Side chain operation with stainless steel bead chain

**Material** [Please select from ShadeTech fabric list or contact us for help]

**Accessories\***  a) Fabric enclosed\*/ 22mm diameter aluminium\* hem-bar

b) Continuous mounting profile

b) Lift assist springs for blind size greater than 3.5 m2

c) Chain retainer (recommended to comply with BS EN 13120:2009) to be installed min 150cm above floor level.

\*There are several different accessory options available e.g. hem bar styles, cassettes, fascia’s, guidewires etc. Please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice.