**Silent Gliss 3000 Cord Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 3000 Cord Operated Curtain Track System**, max width 6 metres, max curtain weight 15kg.** (Can be joined using connecting bridge 3620 subject to weight considerations).

**Finish** White (RAL 9016 gloss) and Black (RAL9005 Satin) powdercoat finish as standard, also available in antique bronze, gold, grey and satin silver anodised.

**Operation** Manual Cord Operation

**Accessories** a) option of ceiling fix or wall brackets

b) cord retainer installed at least 150cm above floor level

c) can be bent, min. standard radius 200mm – please contact technical dept. for advice

Please contact technical@waverley.co.uk or 01252 737973 for advice