**Silent Gliss 5600 Electrically Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 5600 Electrically Operated Curtain Track System, **max width 25 metres, max curtain weight 65kg**

**Finish** White (RAL 9016 Gloss) powdercoat and Satin silver anodised finish as standard

**Operation** Electrically operated with 230v/24v quiet motor, with hard-wired switching/ volt-free signal from 3rd party control system/ radio remote control system with wireless wall switch or hand-held remotes \*. Equipped with ‘Touch and Go’ facility and integrated manual override operation.

**Accessories** a) roller gliders for smooth operation

b) option of top-fix or face fix brackets

c) option of recess profile for flush installations

d) can be bent, standard radius 250mm and 500mm for recess profile; gradual curves available – please call technical advice line

e) option of 60mm/80mm\* Wave glider cord or 60mm/80mm\* Wave roller glider cord (recommended for heavy curtains)

\*Delete as appropriate – please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice