**Silent Gliss 6870 Hand Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 6870 Hand Operated Curtain Track System, **max width 6 metres.** (Can be joined using connecting bridge 3802 subject to weight considerations).

**Finish** White (RAL 9016 gloss) and Black (RAL9005 Satin) powdercoat finish as standard, also available in antique bronze, gold and satin silver anodised.

**Operation** Manual Hand Operation

**Accessories** a) option of ceiling fix or wall brackets

b) 60mm/80mm\* pitch glider cord

c) option of 60mm/80mm\*pitch roller glider cord for heavier curtains.

d) 11230 recess profile\*

e) can be bent, standard radius 260mm; (500mm if used with recess profile) gradual curves available – please call technical advice line

\*Delete as appropriate – please contact technical@waverley.co.uk or 01252 737973 for advice