**Silent Gliss 2700 Panel Glide System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 2700 Panel Glide System**. Max Drop 4m. Max weight 200g per roller glider.**

**Finish** White (RAL 9016 Gloss) powdercoat finish as standard

**Operation** Hand Drawn operation

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories**  a) \* 2-channel, 3-channel, 4-channel or 5-channel profile

b) \*draw rod

c) arranged to stack on right, left or split-draw

\*Delete as appropriate – please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice