**Silent Gliss 4770 Dim-out Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Pproved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 4770 Medium Motorised Dim-out Blind System,

**Max size 2.2m wide x 2.4m high (or 5.3m2). Min width 65cm or 82cm depending on motor choice.** (Please contact us for advice).

**Finish** White (RAL 9016 Gloss) or Black (RAL 9005 Satin) as standard

**Operation** Electrically operated with 230v Hardwired motor\* or 230v radio motor with integrated receiver for use with 9940 series controls (Wall switch, hand-held remotes etc)\*

**Material** [Please select from fabric list below or contact us for help]

**Puma** (PVC/Fibreglass) FR blackout fabric

**Mercuro B** (100% polyester acrylic-coated) FR blackout fabric

**Moon** (100% Polyester Trevira CS Acrylic-coated) FR blackout fabric

**Accessories**  a) 90mm square headbox with hinged front cover

b) 40mm x 24.5mm ZIP side channels

\*Delete as appropriate – please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice