**Silent Gliss 4900 Spring Operated Roller Blind System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 490 Spring Operated Roller Blind System, **Max size 2m wide x 3m high (max 6 m2). Min width 30cm**

**Finish** Steel brackets and extruded aluminium hembar inWhite (RAL 9016 Gloss) powdercoat finish as standard with Child Safe Pull Ball set

**Operation** Manual hand operation

**Material** [Please select from Silent Gliss fabric range or contact us for help]

**Accessories** a) 32mm diameter roller tube

b) option of adjustable stop controller

c) option of side guide wires

Please contact technical@waverley.co.uk or 01252 737973 for advice