**Weinor Pergotex II Retractable Pergola Awning System**

**Manufacturer** Weinor – www.weinor.com

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Weinor Pergotex II Retractable Pergola Awning System, with integrated drainage system. **Max size 7m wide x 6.5m projection**

**Finish** All hardware in powdercoat finish to RAL….(choice of 47 standard colours selected from Weinor range)

**Operation** Electrically operated with 230v Hardwired motor\* or 230v radio motor with integrated receiver for use with BiEasy series controls (Wall switch, hand-held remotes, Wind & Sun sensor, motion sensors etc)\*

**Material** Fabric to be Pergona Classic PVC Awning material (Waterproof) from Weinor fabric collection

**Accessories** a) 115mm square front posts with integrated downpipes

b) option of integrated LED lights to cross members

c) option of Tempura heating system

\*Delete as appropriate – please contact technical@waverley.co.uk or 01252 737973 for advice