**Silent Gliss 1080 Hand Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 1080 Hand Operated Curtain Track System, **max profile length is 6 metres.** (Can be joined using connecting bridge 3620 subject to weight considerations).

**Finish** White (RAL 9016 gloss) and Black (RAL9005 Satin) powdercoat finish as standard, also available in antique bronze, gold, cream and satin silver anodised

**Operation** Manual Hand Drawn Operation

**Accessories** a) available with face fix or top fix brackets

b) can be bent, minimum 100mm radius

Please contact [technical@waverley.co.uk](mailto:technical@waverley.co.uk) or 01252 737973 for advice