**Silent Gliss 1280 Hand Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 1280 Hand Operated Curtain Track System, **max profile length 6 metres. metres** (Can be joined using connecting bridge 3620 subject to weight considerations).

**Finish** White (RAL 9016 gloss) powdercoat finish as standard

**Operation** Manual Hand Drawn Operation

**Accessories** a) available with face fix or top fix brackets

b) roller gliders as standard for ease of operation

c) option of overlap arm to avoid light leakage when curtains configured as a pair

d) can be bent, standard 200mm radius; gradual curves available – please call technical advice line

\*Delete as appropriate – please contact technical@waverley.co.uk or 01252 737973 for advice