**Silent Gliss 3900 Cord Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 3900 Cord Operated Curtain Track System, **max width 12 metres, max curtain weight 20kg**

**Finish** White (RAL 9016) powdercoat finish as standard

**Operation** Manual Cord Operation

**Accessories** a) roller gliders for smooth operation

b) option of ceiling fix or wall brackets

c) cord retainer installed at least 150cm above floor level

d) can be bent, standard radius 200mm; gradual curves available – please call technical advice line

e) metal overlap arm to prevent light leakage

Please contact technical@waverley.co.uk or 01252 737973 for advice