**Silent Gliss 6370 Heavy Duty Cord Operated Curtain Track System**

**Manufacturer** Silent Gliss – www.silentgliss.co.uk

**Approved Installer** Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

Farnham, GU9 9PZ Tel. 01252 737973

www.waverley.co.uk Email. sales@waverley.co.uk

**Reference** Silent Gliss 6370 Heavy Duty Cord Operated Curtain Track System, **max width 15 metres, max curtain weight 70kg.**

**Finish** Satin silver finish as standard

**Operation** Manual Cord Operation

**Accessories** a) roller gliders for smooth operation

b) option of wall brackets (direct ceiling fix preferred)

c) cord retainer installed at least 150cm above floor level

d) can be bent, standard radius 500mm; gradual curves available – please call technical advice line

Please contact technical@waverley.co.uk or 01252 737973 for advice